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Specifications 
	Model No.
	K-180KGMD

	Product Name
	180kgs Double Door MagLock

	

	Lock Size
	336Lx31Wx20.5H(mm)

	Holding Force
	180KGS(350LBS)*2

	Input Voltage
	DC12V (Optional DC24V)

	Current
	12V/160mA(±10%);

	Suitable
	Wooden Door, Metal Door

	Surface Temp
	≤+20℃

	Operating Temp
	-20℃~+55℃(-4—131°F)

	Humidity
	0~90%(non-condensing)

	Cover Finish
	Anodized aluminum

	Lock Finish
	Zinc

	Armature Plate Finish
	Zinc

	Packing Information

	Unit Weight
	2KG

	Standard Package
	6PCS/Carton

	Carton Weight
	12KGS


